1. Download BLE Debugger in Android Phone.
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2. Connect BLE of camera, Then connect to service in the APP.
Click Link Loss and send command
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3. Below is the command list. 
[bookmark: _GoBack]For example 0x00 is for start recording function.


enum _USER_EVENT
{
    USER_STARTREC_EVENT,//record video           //0
    USER_STOPREC_EVENT,//stop video             //1
    USER_PHOTO_EVENT,//take photo              //2
    USER_WIFI_EVENT,//turn on/off wifi           //3
    USER_PWOFF_EVENT,//power off                  //4
    USER_DISC_DEV_EVENT,//Discovery equipment //5
    USER_EVENT_ID_MAX
};
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